## MathAudio Microphone EQ Help

# Welcome to the MathAudio Microphone EQ Help!

## MathAudio Microphone EQ Plug-in

- Linearizes the frequency response of microphones (removes peaks and dips) with the help of a measurement microphone.
- Compares two vocal microphones and converts the sound of the first microphone to the sound of the second microphone.
- Transforms a pair of identical (same model) microphones to a matched pair of microphones for stereo recording.
- Supports microphone calibration files.
- Transforms the sound of a measurement microphone to the sound of an ideal measurement microphone by means of utilizing the microphone calibration file.
- Suitable for real-time applications.
- Applies 64-bit signal path throughout.
- Supports full range of sample rates from 44.1 kHz up to 384 kHz. All sample rates are supported without resampling to avoid any possible loss in quality.
- Supports automatic scaling for 4k monitors. Supports manual window resizing (drag the bottom right corner of the window).
- Supports VST, VST3, CLAP on Windows and AU, VST, VST3, CLAP on Mac.

## System Requirements

MathAudio Microphone EQ VST/VST3:

- Platforms: Windows 10 or later and macOS 10.13 or later.
- VST* compatible host software (Reaper, Cubase, Studio One, etc).

MathAudio Micropnone EQ AU:

- Platforms: macOS 10.13 or later.
- AU** compatible host software (Logic, Garageband, Reason, etc).

MathAudio Microphone EQ CLAP:

- Platforms: Windows 10 or later and macOS 10.13 or later.
- CLAP*** compatible 64-bit host software (Bitwig Studio, Reaper, FL Studio, MultitrackStudio, etc).

* VST is a trademark and software of Steinberg Media Technologies GmbH.
** Audio Unit is a trademark of Apple, Inc.
*** CLAP (CLever Audio Plug-in API) is an open plug-in standard.

## Contents

### Welcome to the MathAudio Microphone EQ Help

How to improve the frequency response of your microphone Registration