## MathAudio Reverb Help

# Welcome to the MathAudio Reverb Help!

## MathAudio Reverb Plug-in

- Applies an algorithmic method of echo synthesis.
- Avoids the metallic timbre of conventional algorithmic reverbs.
- Provides a sense of space and natural depth.
- Works with zero latency. Suitable for live performances and direct monitoring.
- Applies 64-bit signal path throughout.
- Supports full range of sample rates from 44.1 kHz up to 384 kHz (88.2 kHz or higher recommended).
- Supports automatic scaling for 4k monitors. Supports manual window resizing (drag the bottom right corner of the window).
- Supports VST, VST3, CLAP on Windows and AU, VST, VST3, CLAP on Mac.

## System Requirements

MathAudio Reverb VST/VST3:

- Platforms: Windows 10 or later and macOS 10.13 or later
- VST* compatible host software (Reaper, Cubase, Nuendo, etc).

MathAudio Reverb AU:

- Platforms: macOS 10.13 or later
- AU** compatible host software (Logic, Garageband, etc).

MathAudio Reverb CLAP:

- Platforms: Windows 10 or later and macOS 10.13 or later.
- CLAP*** compatible 64-bit host software (Bitwig Studio, Reaper, FL Studio, MultitrackStudio, etc).

* VST is a trademark and software of Steinberg Media Technologies GmbH.
** Audio Unit is a trademark of Apple, Inc.
***CLAP (CLever Audio Plug-in API) is an open plug-in standard.

## Contents

### Welcome to the MathAudio Reverb Help

MathAudio Reverb controls Registration